**DEBRA THANA SKS MAHAVIDYALAYA CHAKSHYAMPUR, DEBRA, PASCHIM MEDINIPUR-721124**

**PHONE-** 03222-243400

[**www.debracollege.ac.in**](http://www.debracollege.ac.in/)

**Notice Inviting quotation**

**Tender No- dtsksm/NIT60/24 dated:28.08.2024**

Sealed quotations are hereby invited from reputed suppliers/agencies with suitable credentials for supply and/or installation of miscellaneous items/works. Detailed list is available in the website [www.debracollege.ac.in](http://www.debracollege.ac.in/) and in the college notice board. Rate must be inclusive of all taxes.

* Last date and time for submission of quotation: 04.09.2024 till 1p.m.
* Date & Time of opening of quotation: 04.09.2024 at 3.00 p.m

(Dr. Rupa Dasgupta) Principal

**List (Tender format to be submitted in letterhead of the company/supplier)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Sl. No.** | **Item/make/Description** | **Unit** | **Rate /Unit** |
| 1. | **Lab. Table:** |  |  |
|  | Frame made up of Akashmani/Neem wood, Made by 18 mm ply (No Particle/mdf board), middle shelve, | Sq Ft |
|  | outside laminate (1mm) inside paint. Measurement of table top to top |  |
| 2. | **Teachers desk :** |  |
|  | Frame made up of Akashmani/Neem wood ,Made by 18 mm ply (No Particle/mdf board), front ply, inside | Sq Ft |
|  | keyboard, drawer, outside laminate ( 1mm) inside paint. Measurement |  |
|  | top to top |  |
| 3. | **Aluminum Sliding Window:** | Sq Ft |
|  | Fitting & fixing of sliding window with |  |
|  | Aluminium section with glass |  |
| 4. | **File Cabinet/Store :** |  |
|  | Made by 18 mm ply (No Particle/mdf board), front cover by | Sq Ft |
|  | 18mm block board/Glass, inside shelve outside laminate inside |  |
|  | paint with lock and fittings .Measurement front to front. |  |
| 5. | **Open Rack :** |  |
|  | Made by 18 mm ply (No Particle/mdf board) with shelve | Sq Ft |
|  | Measurement front to front. |  |
|  | **Wooden Chair :** | Pc |
| 6. | Made by Neem/Akasmoni wood |  |
|  | **Notice Board :** |  |
| 7. | Made by 18 mm ply, laminate, soft board, velvet, covering by glass. | SqFt |
| 8. | **Window curtain:**  Curtain Fitting with steel rod and wooden bracket: | Pc |
| 9.  10.  11. | Fitting and fixing of Precast pre polished chequered tiles with all materials ( approximate area 1000 sq ft  Table top toughened Glass 6 mm, 8mm  Desktop Configuration (Required Qty. 1)  Processor: Core i5 12 generation (12 MB cache, 10 Cores, 12 threads up to 5GHz turbo)  RAM: 16GB (1x16), DDR4, 3200 MT/s  SSD: 1TB  GPU: NVIDIA GeForce RTX 3050 4GB GDDR6 Dedicated Graphic | Sq Ft  Sq Ft  Per Unit |